Socket Programming 2

Sharan Narasimhan, CS20MTECH14003

October 4th, 2020

# 1. Foreword to Evaluators:

For Task 1, I have implemented the source code up to the DNS response processing section. So it is only able the send the DNS packet to server and retrieve the unprocessed response. I had to refer to online resources for the theory and have used the two links the TA provided us. I also had to refer to few DNS tutorials in order to understand certain code segments. All these sources have been referenced wherever needed. I have briefly documented whatever I have learnt from these online tutorials as well.

For Task 2, I have made use of the FD API and the select() function in order facilitate multi socket servicing. All online documentation/tutorials used have been referenced. Code comments have been added for explanation and I have discussed only critical parts of the code in the report.

# 2. Simple DNS Client using UDP

In *Line 35-49*, I have used the same methods used in the earlier assignments to initialise the UDP Client and configure the DNS Server Address. Using an online IP to Hex tool, I obtained the hex form of the IP for the IITH DNS server (declared in *Line 48*).

Text

Description automatically generated

Figure 2.1

A DNS packet consists of 5 sections, Header, Question, Answer (also contains ‘Response’), Authority and Additional.

Header:

The header consists of three lines: Random Identifier/ XID (2 Bytes), OPCODE (2 Bytes) and Question Field (2 Bytes).

The XID is a randomly generated 16 bit field created by the client that is used to identify the particular DNS query/response. In the response from DNS Server, the XID should match the sending XID to convey that the response is for the particular query.

The OPCODE is a 16 bit field that consists of various flags/options available for the DNS query. Only the ‘RD’ flag was set to 1, to denote that Recursion method is desired over the iterative method. Thus the corresponding hex code is 0100.

Lastly, the question field conveys how many IPs we want to resolve. So in this case the corresponding 16 bit code is: 0001 0000 0000 0000. The structure *dns\_header* was declared to store the header information (Figure 2.2)

Text

Description automatically generated

Figure 2.2

A header object of type *dns\_header* was declared and was initialised appropriately with the *XID, OPCODE/Flags* and *No. of questions*. (Figure 2.3)

Text

Description automatically generated

Figure 2.3

Question:

The question consists 2 sections: *QNAME* (variable length), *QCLASS* (1 Byte) and *QTYPE* (1 Byte).

The *QNAME* consists of the name of the domain (e.g. “facebook” in “www.facebook.com” in ASCII form followed by a field with 3 characters corresponding to .COM and continues till the first 0 Byte is read. This *QNAME* field first needs to be pre-processed to the DNS name format (explained later)

*QCLASS* is set to IN meaning “Internet” and *QTYPE* corresponds to 1 of the 4 types of record responses requested, ‘A’ in this case for Authoritative. The final 16 bit code is 0001 0001. The structure *dns\_question* was defined to store all the information for a DNS question. (Figure 2.4)

A picture containing text

Description automatically generated

Figure 2.4

An object question was declared and was initialised appropriately with the domain name, QTYPE and QCLASS. The domain name must first pre-processed to suite the DNS Name format. E.g. [www.facebook.com](http://www.facebook.com) must get transformed to 3www8facebook3com0. I was not able to implement this pre-process function so have directly hardcoded this while declaring the object:

Graphical user interface, text

Description automatically generated

Figure 2.5

The packet length is first computed in *Line 68*. We need to add an extra 2 Bytes for the first extra byte store ‘3’ and the last null byte storing ‘0’ in the processed hostname. Memory is allocated and the address is stored in the pointer packet. We then proceed to copy the Header and Question data incrementally into the memory space as shown:

Text

Description automatically generated

Figure 2.6

We then initialise an object response and allocation its memory with 0’s. The packet is sent and the number of bytes received stored in the variable bytes as shown:

Text

Description automatically generated

Figure 2.7

The output obtained after compiling and executing the program is shown below:

Graphical user interface, text, application, website

Description automatically generated

Figure 2.2

The online tutorial that was mainly used: <https://w3.cs.jmu.edu/kirkpams/OpenCSF/Books/csf/html/UDPSockets.html>.

For more theory on the DNS header and its corresponding flags I used: https://www2.cs.duke.edu/courses/fall16/compsci356/DNS/DNS-primer.pdf

# 3. Multi-Client Chat Server using select()

Instead of using multi-threading, It seemed more effective to use the select() function. Sockets are treated identically to files (referenced by file descriptors) with respect to the kernel. This enables select() to be used to fetch and push information into sockets whenever an FD ‘event’ occurs.